Installation:

System requirements:
Win2000 or WinXP

1) Connect USB-Piezo-Controller to the computer
Computer recognizese new USB-Hardware

2) The computer automatically is looking and 
asking for the path of the driver.
It is on the CD the following path:
English\Software Controller CU30\Driver
3) To start the controller software copy CU30-0.exe from
the CD on the computer and double click it to start the programm.


Directories:

CU30_Wrapper:
- C/C++ wrapper project for the CU30.dll driver DLL.

CU30_Delphi:
- Delphi 7.0 project.

CU30_LabView:
- LabView 8.0 Driver


